{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.036","0.060","0.060"]
["","Aquecimento","","Nom.","kW","0.036","0.060","0.060"]
["Dimensões","Unidade","","Altura","mm","200","200","200"]
["","","","Largura","mm","750","1150","1150"]
["","","","Profundidade","mm","620","620","620"]
["Peso","Unidade","","","kg","21","28","28"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","8.7","15.8","16.0"]
["","","","Médio","m³/min","8.0","14.6","14.8"]
["","","","B","m³/min","7.3","13.3","13.5"]
["","","Aquecimento","Alto","m³/min","8.7","15.8","16.0"]
["","","","Médio","m³/min","8.0","14.6","14.8"]
["","","","B","m³/min","7.3","13.3","13.5"]
["","Pressão estática disponível","","Nom.","Pa","30","40","40"]
["Nível de potência sonora","Arrefecimento","","","dBA","53","55","56"]
["","Aquecimento","","","dBA","53","55","56"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","35","38","38"]
["","","","Médio","dBA","33","35","35"]
["","","","B","dBA","27","30","30"]
["","Aquecimento","","Alto","dBA","35","38","38"]
["","","","Médio","dBA","33","35","35"]
["","","","B","dBA","27","30","30"]
["Ligações de tubagem","Líquido","","DE","mm","6.35","6.35","6.35"]
["","Gás","","DE","mm","9.50","12.70","12.70"]
["","Esgoto","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Acessórios standard","Installation manual","","","","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8"]
["","Operation manual","","","","1","1","1"]
["","Clamp metal","","","","1","1","1"]
["","Clamps","","","","6","6","6"]
["","Drain hose","","","","1","1","1"]
["","Air filter","","","","1","1","1"]
["","Insulation for fitting","","","","1","1","1"]
["","Screws for duct flanges","","","","1","1","1"]
["","Sealing material","","","","2","2","2"]
["","Sealing pad","","","","1","1","1"]
["","Washer fixing plate","","","","4","4","4"]
["Alimentação elétrica","Fase","","","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240"]