{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Nível de pressão sonora","Aquecimento","Alto","dBA","35","35","38","38"]
["","","Médio","dBA","33","33","35","35"]
["","","B","dBA","27","27","30","30"]
["","Arrefecimento","Medium","dBA","33","33","35","35"]
["","","B","dBA","27","27","30","30"]
["","","Alto","dBA","35","35","38","38"]
["Acessórios standard","Manual de instalação","","","1","1","1","1"]
["","Manual de funcionamento","","","1","1","1","1"]
["","Isolamento para instalação","","","1","1","1","1"]
["","Chapa vedante","","","1","1","1","1"]
["","Braçadeira de metal","","","1","1","1","1"]
["","Tubo flexível de drenagem","","","1","1","1","1"]
["","Anilha para o suporte do gancho","","","8","8","8","8"]
["","Material vedante","","","2","2","2","2"]
["","Braçadeiras","","","6","6","6","6"]
["","Chapa de fixação da anilha","","","4","4","4","4"]
["","Parafusos para flanges de conduta","","","1","1","1","1"]
["","Filtro de ar","","","1","1","1","1"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gás","OD","mm","9.50","9.50","12.70","12.70"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Power input","Arrefecimento","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Aquecimento","Nom.","kW","0.036","0.036","0.060","0.060"]
["Nível de potência sonora","Arrefecimento","","dBA","53","53","55","56"]
["","Aquecimento","","dBA","53","53","55","56"]
["Dimensões","Unidade","Width","mm","750","750","1,150","1,150"]
["","","Depth","mm","620","620","620","620"]
["","","Altura","mm","200","200","200","200"]
["Peso","Unidade","","kg","21","21","28","28"]
["Ventilador","Pressão estática disponível","Nom.","Pa","30","30","40","40"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frequência","","Hz","50","50","50","50"]
["","Tensão","","V","220-240","220-240","220-240","220-240"]