{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","35.0","35.0","","38.0"]
["","","","Médio","dBA","33.0","33.0","","35.0"]
["","","","B","dBA","27.0","27.0","","30.0"]
["","Arrefecimento","","Medium","dBA","33.0","33.0","","35.0"]
["","","","B","dBA","27.0","27.0","","30.0"]
["","","","Alto","dBA","35.0","35.0","","38.0"]
["Acessórios standard","Manual de instalação","","","","1","1","","1"]
["","Manual de funcionamento","","","","1","1","","1"]
["","Isolamento para instalação","","","","1","1","","1"]
["","Chapa vedante","","","","1","1","","1"]
["","Braçadeira de metal","","","","1","1","","1"]
["","Tubo flexível de drenagem","","","","1","1","","1"]
["","Anilha para o suporte do gancho","","","","8","8","","8"]
["","Material vedante","","","","2","2","","2"]
["","Braçadeiras","","","","6","6","","6"]
["","Chapa de fixação da anilha","","","","4","4","","4"]
["","Parafusos para flanges de conduta","","","","1","1","","1"]
["","Filtro de ar","","","","1","1","","1"]
["Ligações de tubagens","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gás","","OD","mm","9.50","9.50","","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Arrefecimento","","Nom.","kW","0.036","0.036","","0.060"]
["","Aquecimento","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Arrefecimento","","","dBA","53.0","53.0","","56.0"]
["","Aquecimento","","","dBA","53.0","53.0","","56.0"]
["Dimensões","Unidade","","Largura","mm","750","750","","1,150"]
["","","","Profundidade","mm","620","620","","620"]
["","","","Altura","mm","200","200","","200"]
["Peso","Unidade","","","kg","21","21","","28"]
["Ventilador","Pressão estática disponível","","Nom.","Pa","30","30","","40"]
["","Caudal de ar","Aquecimento","Alto","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","B","m³/min","7.3","7.3","","13.5"]
["","","Arrefecimento","B","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Alto","m³/min","8.7","8.7","","16.0"]
["Power supply","Fase","","","","1~","1~","","1~"]
["","Frequência","","","Hz","50","50","","50"]
["","Tensão","","","V","220-240","220-240","","220-240"]
["Notas","","","","","(1) - Consulte o esquema separado para conhecer os dados eléctricos","(1) - Consulte o esquema separado para conhecer os dados eléctricos","","(1) - Consulte o esquema separado para conhecer os dados eléctricos"]
["Potência nominal","Arrefecimento","","Nom.","kW","","","0.060"]
["","Aquecimento","","Nom.","kW","","","0.060"]
["Dimensões","Unidade","","Altura","mm","","","200"]
["","","","Largura","mm","","","1150"]
["","","","Profundidade","mm","","","620"]
["Peso","Unidade","","","kg","","","28"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","","","15.8"]
["","","","Médio","m³/min","","","14.6"]
["","","","B","m³/min","","","13.3"]
["","","Aquecimento","Alto","m³/min","","","15.8"]
["","","","Médio","m³/min","","","14.6"]
["","","","B","m³/min","","","13.3"]
["","Pressão estática disponível","","Nom.","Pa","","","40"]
["Nível de potência sonora","Arrefecimento","","","dBA","","","55.0"]
["","Aquecimento","","","dBA","","","55.0"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","","38.0"]
["","","","Médio","dBA","","","35.0"]
["","","","B","dBA","","","30.0"]
["","Aquecimento","","Alto","dBA","","","38.0"]
["","","","Médio","dBA","","","35.0"]
["","","","B","dBA","","","30.0"]
["Ligações de tubagem","Líquido","","DE","mm","","","6.35"]
["","Gás","","DE","mm","","","12.70"]
["","Esgoto","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Acessórios standard","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Air filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Alimentação elétrica","Fase","","","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","","50"]
["","Tensão","","","V","","","220-240"]