{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60F2VEB / RXS60F4V1B"]
["Capacidade de arrefecimento","Mín.","","kW","1.7"]
["","Máx.","","kW","6.5"]
["","Nom.","","kW","6.0 (2)"]
["Piping connections","Liquid","OD","mm","6.35"]
["","Gás","OD","mm","12.7"]
["","Drain","OD","mm","VP20 (diâmetro externo 26, diâmetro interno 20)"]
["Eficiência nominal","Annual energy consumption","","kWh","1,030"]
["","EER","","","2.91 (1)"]
["","COP","","","3.21 (1)"]
["","Diretiva de etiqueta da energia","Arrefecimento","","C"]
["","","Aquecimento","","C"]
["Capacidade de aquecimento","Nom.","","kW","7.0 (3)"]
["","Mín.","","kW","1.7"]
["","Máx.","","kW","8.0"]
["Notas","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - Arrefecimento: temp. interior: 27°CBs, 19,0°CBh; temp. exterior 35°CBs; 24°CBh; comprimento equivalente de tubagem: 5m"]
["","","","","(3) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 5m"]
["","","","","(4) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]