{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25L2V1B","FDXS35F2VEB / RXS35L2V1B","FDXS60F2VEB / RXS60L2V1B"]
["Capacidade de arrefecimento","Mín.","","kW","1.3","1.4","1.7"]
["","Máx.","","kW","3.0","3.8","6.5"]
["","Nom.","","kW","2.4","3.4","6.0"]
["Ligações de tubagens","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gás","OD","mm","9.5","9.5","12.7"]
["","Drain","OD","mm","VP20 (diâmetro externo 26, diâmetro interno 20)","VP20 (diâmetro externo 26, diâmetro interno 20)","VP20 (diâmetro externo 26, diâmetro interno 20)"]
["Eficiência nominal","Annual energy consumption","","kWh","325","530","1,030"]
["","EER","","","3.69","3.21","2.91"]
["","COP","","","4.00","3.48","3.21"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A","C"]
["","","Aquecimento","","A","B","C"]
["Capacidade de aquecimento","Nom.","","kW","3.2","4.0","7.0"]
["","Mín.","","kW","1.3","1.4","1.7"]
["","Máx.","","kW","4.5","5.0","8.0"]
["Notas","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","(3) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","(3) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","(3) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]