{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS60F2VEB / FDXS60F2VEB / RZQG125L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG125L8Y1B (Archived)"]
["Arrefecimento ambiente","SEER","","","4.80","4.8","5.10"]
["","Consumo anual de energia","","kWh/a","496","496","652"]
["","Capacidade","Pdesign","kW","6.80","6.8","9.50"]
["","Classe de eficiência energética","","","B","B","B"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","6.00","6","10.74"]
["","SCOP/A","","","3.80","3.8","3.80"]
["","Classe de eficiência energética","","","A","A","A"]
["","Consumo anual de energia","","kWh/a","2,211","2,211","3,957"]
["Notas","","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["Arrefecimento ambiente","Classe de eficiência energética","","","","","","B","B","B"]
["","Capacidade","Pdesign","kW","","","","9.5","12","12.00"]
["","SEER","","","","","","5.1","5.1","5.10"]
["","Consumo anual de energia","","kWh/a","","","","652","824","824"]
["Aquecimento ambiente (clima médio)","Classe de eficiência energética","","","","","","A","A","A"]
["","Capacidade","Pdesign","kW","","","","10.74","12.71","11.30"]
["","SCOP/A","","","","","","3.8","3.8","3.80"]
["","Consumo anual de energia","","kWh/a","","","","3957","4683","4164"]
["Gama de eficiência energética","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Outdoor unit","","","","","","","","","RZQG125L8Y1"]