{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQSG100L9V1B","FDXS60F2VEB / FDXS60F2VEB / RZQSG125L9V1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQSG125L9V1B"]
["Arrefecimento ambiente","SEER","","","4.80","4.80","4.80"]
["","Consumo anual de energia","","kWh/a","693","875","875"]
["","Capacidade","Pdesign","kW","9.50","12.00","12.00"]
["","Classe de eficiência energética","","","B","B","B"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","7.10","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80"]
["","Classe de eficiência energética","","","A","A","A"]
["","Consumo anual de energia","","kWh/a","2,616","2,800","2,800"]
["Notas","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]