{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Nível de pressão sonora","Aquecimento","Alto","dBA","38"]
["","","Médio","dBA","36"]
["","","B","dBA","30"]
["","Arrefecimento","Médio","dBA","36"]
["","","B","dBA","30"]
["","","Alto","dBA","38"]
["Acessórios standard","Manual de instalação","","","1"]
["","Manual de funcionamento","","","1"]
["","Isolamento para instalação","","","1"]
["","Chapa vedante","","","1"]
["","Braçadeira de metal","","","1"]
["","Tubo flexível de drenagem","","","1"]
["","Anilha para o suporte do gancho","","","8"]
["","Material vedante","","","2"]
["","Braçadeiras","","","6"]
["","Chapa de fixação da anilha","","","4"]
["","Parafusos para flanges de conduta","","","1"]
["","Filtro de ar","","","1"]
["Ligações de tubagem","Líquido","DE","mm","6.35"]
["","Gás","DE","mm","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)"]
["Potência nominal","Arrefecimento","Nom.","kW","0.060"]
["","Aquecimento","Nom.","kW","0.060"]
["Nível de potência sonora","Arrefecimento","","dBA","55"]
["","Aquecimento","","dBA","55"]
["Dimensões","Unidade","Largura","mm","1,150"]
["","","Profundidade","mm","620"]
["","","Altura","mm","200"]
["Peso","Unidade","","kg","30.0"]
["Ventoinha","Pressão estática disponível","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frequência","","Hz","50/60"]
["","Nome","","","VE"]
["","Tensão","","V","220-240"]
["Notas","","","","(1) - Quando ligado com unidade exterior de multi-sistema, consulte as especificações da unidade exterior multi a ser ligada."]