{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB9","FFA35A2VEB9","FFA50A2VEB9","FFA60A2VEB9"]
["Envolvente","Material","","","","Chapa de aço galvanizado","Chapa de aço galvanizado","Chapa de aço galvanizado","Chapa de aço galvanizado"]
["Dimensões","Unidade","","Altura","mm","260","260","260","260"]
["","","","Largura","mm","575","575","575","575"]
["","","","Profundidade","mm","575","575","575","575"]
["Peso","Unidade","","","kg","16.0","16.0","17.5","17.5"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","9.0","10.0","12.7","14.5"]
["","","","Médio","m³/min","8.0","8.5","10.9","12.5"]
["","","","B","m³/min","6.5","6.5","8.6","9.5"]
["","","Aquecimento","Alto","m³/min","9.0","10.0","12.7","14.5"]
["","","","Médio","m³/min","8.0","8.5","10.9","12.5"]
["","","","B","m³/min","6.5","6.5","8.6","9.5"]
["Nível de potência sonora","Arrefecimento","","","dBA","48.0","51.0","56.0","60.0"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","31.0","34.0","39.0","43.0"]
["","","","Médio","dBA","28.5","30.5","34.0","40.0"]
["","","","B","dBA","25.0","25.0","27.0","32.0"]
["","Aquecimento","","Alto","dBA","31.0","34.0","39.0","43.0"]
["","","","Médio","dBA","28.5","30.5","34.0","40.0"]
["","","","B","dBA","25.0","25.0","27.0","32.0"]
["Ligações de tubagem","Líquido","","DE","mm","6","6","6","6"]
["","Gás","","DE","mm","9.52","9.52","12.70","12.70"]
["","Esgoto","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Painel decorativo","Modelo","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Cor","","","","Branco (N9.5)","Branco (N9.5)","Branco (N9.5)","Branco (N9.5)"]
["","Dimensões","","Altura","mm","46","46","46","46"]
["","","","Largura","mm","620","620","620","620"]
["","","","Profundidade","mm","620","620","620","620"]
["","Peso","","","kg","2.8","2.8","2.8","2.8"]
["Painel decorativo 2","Modelo","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Cor","","","","Prateado","Prateado","Prateado","Prateado"]
["","Dimensões","","Altura","mm","46","46","46","46"]
["","","","Largura","mm","620","620","620","620"]
["","","","Profundidade","mm","620","620","620","620"]
["","Peso","","","kg","2.8","2.8","2.8","2.8"]
["Painel decorativo 3","Modelo","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Cor","","","","Branco (RAL9010)","Branco (RAL9010)","Branco (RAL9010)","Branco (RAL9010)"]
["","Dimensões","","Altura","mm","55","55","55","55"]
["","","","Largura","mm","700","700","700","700"]
["","","","Profundidade","mm","700","700","700","700"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Painel decorativo 4","Modelo","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Cor","","","","Branco (RAL9010)","Branco (RAL9010)","Branco (RAL9010)","Branco (RAL9010)"]
["","Dimensões","","Altura","mm","55","55","55","55"]
["","","","Largura","mm","700","700","700","700"]
["","","","Profundidade","mm","700","700","700","700"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","BRC7EB530 (painel padrão), BRC7F530W (painel branco), BRC7F530S (painel cinzento)","BRC7EB530 (painel padrão), BRC7F530W (painel branco), BRC7F530S (painel cinzento)","BRC7EB530 (painel padrão), BRC7F530W (painel branco), BRC7F530S (painel cinzento)","BRC7EB530 (painel padrão), BRC7F530W (painel branco), BRC7F530S (painel cinzento)"]
["","Controlo remoto por cabo","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Acessórios standard","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Alimentação elétrica","Fase","","","","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240"]