{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-F"]
[]
[]
[]
[]
["","","","","FFQ60B9V1B / RXS60F3V1B","FFQ60B9V1B / RXS60F4V1B"]
["Capacidade de arrefecimento","Nom.","","kW","5.80 (3)","5.80 (3)"]
["Eficiência nominal","Annual energy consumption","","kWh","1,035","1,035"]
["","EER","","","2.80","2.80"]
["","COP","","","2.81","2.81"]
["","Diretiva de etiqueta da energia","Arrefecimento","","D","D"]
["","","Aquecimento","","D","D"]
["Capacidade de aquecimento","Nom.","","kW","7.00 (4)","7.00 (4)"]
["Notas","","","","(1) - Etiqueta energética: escala de A (mais eficiente) a G (menos eficiente)","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - Consumo anual de energia: baseado na utilização média de 500 horas de funcionamento por ano em plena carga (condições nominais)","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]
["","","","","(3) - Arrefecimento: temp. interior: 27°CBs, 19°CBh; temp. exterior 35°CBs; comprimento de tubagem equivalente: 7,5m; desnível: 0m"]
["","","","","(4) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 7,5m; desnível: 0m"]
["","","","","(5) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]