{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RZQSG71L3V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L9V1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L9V1B","FHQ125CAVEB / RZQSG125L9V1B"]
["Capacidade de arrefecimento","Nom.","","kW","6.8","","","12.0"]
["Arrefecimento ambiente","SEER","","","5.61","5.10","5.10","5.61"]
["","Consumo anual de energia","","kWh/a","424","652","652","749"]
["","Capacidade","Pdesign","kW","6.80","9.50","9.50","12.00"]
["","Classe de eficiência energética","","","A+","B","B","A+"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.90","3.80","3.80","4.01"]
["","Classe de eficiência energética","","","A","A","A","A+"]
["","Consumo anual de energia","","kWh/a","2,727","2,800","2,800","2,654"]
["Eficiência nominal","Annual energy consumption","","kWh","985","","","2,075"]
["","EER","","","3.46","","","2.89"]
["","COP","","","4.00","","","3.62"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","","","C"]
["","","Aquecimento","","A","","","A"]
["Capacidade de aquecimento","Nom.","","kW","7.5","","","13.5"]
["Notas","","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]