{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":16,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Capacidade de arrefecimento","Nom.","","kW","","","6.8","","","","","","","","","13.4"]
["Arrefecimento ambiente","SEER","","","5.10","5.10","6.86","6.95","5.10","5.10","5.10","5.10","6.11","5.10","6.01"]
["","Consumo anual de energia","","kWh/a","467","467","347","343","467","652","652","824","545","652","699"]
["","Capacidade","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","12.00","9.50","9.50","12.00"]
["","Classe de eficiência energética","","","B","B","A++","A++","B","B","B","B","A++","B","A+"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","6.00","6.00","7.60","7.60","6.00","11.30","11.30","12.71","11.30","11.30","14.13"]
["","SCOP/A","","","3.80","3.80","4.32","4.32","3.80","3.80","3.80","3.80","4.61","3.80","4.23"]
["","Classe de eficiência energética","","","A","A","A+","A+","A","A","A","A","A++","A","A+"]
["","Consumo anual de energia","","kWh/a","2,211","2,211","2,463","2,463","2,211","4,164","4,164","4,683","3,432","4,164","4,677"]
["Eficiência nominal","Consumo anual de energia","","kWh","","","890","","","","","","","","","2,025"]
["","EER","","","","","3.82","","","","","","","","","3.31"]
["","COP","","","","","4.13","","","","","","","","","3.63"]
["","Diretiva de etiqueta da energia","Arrefecimento","","","","A","","","","","","","","","A"]
["","","Aquecimento","","","","A","","","","","","","","","A"]
["Capacidade de aquecimento","Nom.","","kW","","","7.5","","","","","","","","","15.5"]
["Notas","","","","","","(1) - Consumo anual de energia de acordo com a directiva de etiquetagem de energia 2002/31/EC","","","","","","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","","","(2) - SEER e SCOP de acordo com a EN 14825","","","","","","","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]