{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L3"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L3V1B"]
["Capacidade de arrefecimento","Nom.","","kW","3.5 (2)"]
["Ligações de tubagens","Liquid","OD","mm","6.35"]
["","Gás","OD","mm","9.5"]
["","Drain","OD","mm","18.0"]
["Eficiência nominal","Annual energy consumption","","kWh","608"]
["","EER","","","2.88 (1)"]
["","COP","","","3.57 (1)"]
["","Diretiva de etiqueta da energia","Arrefecimento","","B"]
["","","Aquecimento","","A"]
["Capacidade de aquecimento","Nom.","","kW","4.0 (2)"]
["","Mín.","","kW","1.4"]
["","Máx.","","kW","5.0"]
["Notas","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]
["","","","","(3) - 220V"]
["","","","","(4) - 230V"]
["","","","","(5) - 240V"]