{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Nível de pressão sonora","Aquecimento","Alto","dBA","46"]
["","","Funcionamento silencioso","dBA","30"]
["","","B","dBA","33"]
["","Arrefecimento","Funcionamento silencioso","dBA","29"]
["","","B","dBA","32"]
["","","Alto","dBA","38"]
["","","Nom.","dBA","36"]
["","Arrefecimento","Nom.","dBA","35"]
["Acessórios standard","Manual de instalação","","","1"]
["","Manual de funcionamento","","","1"]
["","Controle remoto por infravermelhos","","","1"]
["","Pilhas secas AAA","","","2"]
["","Suporte do controle remoto","","","1"]
["","Chapa de montagem","","","1"]
["","Tubo de isolamento do calor (tubo de refrigerante)","","","8"]
["","Filtro de purificação do ar","","","1"]
["","Filtro desodorizante fotocatalítico","","","1"]
["","Tampa lateral","","","2"]
["","Fita de união","","","4"]
["Sistemas de controlo","Infrared remote control","","","ARC433B67"]
["Ligações de tubagens","Liquid","OD","mm","6.35"]
["","Gás","OD","mm","9.5"]
["","Drain","","","18"]
["Sound power level","Arrefecimento","","dBA","53"]
["","Aquecimento","","dBA","59"]
["Dimensões","Unidade","Largura","mm","1,050"]
["","","Profundidade","mm","200"]
["","","Altura","mm","490"]
["Envolvente","Cor","","","Branco amêndoa"]
["Peso","Unidade","","kg","16"]
["Power supply","Fase","","","1~"]
["","Frequência","","Hz","50"]
["","Nome","","","VM"]
["","Tensão","","V","220-240"]
["Notas","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Quando ligado com unidade exterior de multi-sistema, consulte as especificações da unidade exterior multi a ser ligada."]