{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Nível de pressão sonora","Aquecimento","Alto","dBA","42","44","46","39","40","41"]
["","","Funcionamento silencioso","dBA","30","32","34","25","25","26"]
["","","B","dBA","33","35","37","28","28","29"]
["","Arrefecimento","Funcionamento silencioso","dBA","31","33","34","22","22","23"]
["","","B","dBA","34","36","37","25","26","27"]
["","","Alto","dBA","43","45","46","39","40","41"]
["","","Nom.","dBA","38","40","42","34","34","35"]
["","Arrefecimento","Nom.","dBA","39","41","42","33","33","34"]
["Acessórios standard","Manual de instalação","","","1","1","1","1","1","1"]
["","Manual de funcionamento","","","1","1","1","1","1","1"]
["","Controle remoto sem fios","","","1","1","1","1","1","1"]
["","Pilhas","","","2","2","2","2","2","2"]
["","Suporte do controle remoto","","","1","1","1","1","1","1"]
["","Chapa de montagem","","","1","1","1","1","1","1"]
["","Parafuso de fixação para unidade interior","","","","","","2","2","2"]
["","Filtro fotocatalítico de apatite de titânio","","","2","2","2","2","2","2"]
["Sistemas de controlo","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Ligações de tubagens","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gás","OD","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Drain","","","18","18","18","18","18","18"]
["Power input","Arrefecimento","Nom.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Aquecimento","Nom.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Sound power level","Arrefecimento","","dBA","59","60","63","55","56","57"]
["","Aquecimento","","dBA","58","59","62","55","56","57"]
["Dimensões","Unidade","Largura","mm","1,050","1,050","1,050","770","770","770"]
["","","Profundidade","mm","238","238","238","198","198","198"]
["","","Altura","mm","290","290","290","283","283","283"]
["Envolvente","Cor","","","Branco","Branco","Branco","Branco","Branco","Branco"]
["Peso","Unidade","","kg","12","12","12","7","7","7"]
["Power supply","Fase","","","1~","1~","1~","1~","1~","1~"]
["","Frequência","","Hz","50","50","50","50","50","50"]
["","Nome","","","V1","V1","V1","V1","V1","V1"]
["","Tensão","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Acessórios standard","Parafusos de fixação da unidade interior","","","2","2"]
["Notas","","","","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Acessórios standard","Parafusos de fixação da unidade interior (M4 x 12L)","","","","","2"]