{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW (Archived)"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","39","40","41","","46"]
["","","","Médio","dBA","32","33","33","","42"]
["","","","Funcionamento silencioso","dBA","19","19","19","","24"]
["","","","B","dBA","25","25","25","","33"]
["","Arrefecimento","","Médio","dBA","32","33","33","","39"]
["","","","Funcionamento silencioso","dBA","19","19","19","","24"]
["","","","B","dBA","25","25","25","","31"]
["","","","Alto","dBA","39","40","41","","46"]
["Acessórios standard","Manual de instalação","","","","1","1","1","","1"]
["","Manual de funcionamento","","","","1","1","1","","1"]
["","Filtro de ar","","","","2","2","2","","2"]
["","Controle remoto por infravermelhos","","","","1","1","1","","1"]
["","Placa de instalação do controlador remoto","","","","1","1","1","","1"]
["","Saco de parafusos","","","","1","1","1","","1"]
["","Tampa do parafuso","","","","1","1","1","","1"]
["","Pilhas secas AAA","","","","2","2","2","","2"]
["","Precauções gerais de segurança","","","","1","1","1","","1"]
["Fluido frigorigéneo","GWP","","","","675.0","675.0","675.0","","675.0"]
["Sistemas de controlo","Controlo remoto por cabo","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Ligações de tubagem","Líquido","","DE","mm","6.35","6.35","6.35","","6.35"]
["","Gás","","DE","mm","9.50","9.50","9.50","","12.70"]
["","Esgoto","","","","18","18","18","","18"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Aquecimento","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Nível de potência sonora","Arrefecimento","","","dBA","57","57","60","","60"]
["Dimensões","Unidade","","Largura","mm","798","798","798","","798"]
["","","","Profundidade","mm","189","189","189","","189"]
["","","","Altura","mm","295","295","295","","295"]
["Envolvente","Cor","","","","Branco","Branco","Branco","","Branco"]
["Peso","Unidade","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Médio","m³/min","8.7","9.0","9.0","","11.1"]
["","","","B","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Funcionamento silencioso","m³/min","4.5","4.5","4.5","","5.7"]
["","","Arrefecimento","B","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Médio","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Alto","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Funcionamento silencioso","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Fase","","","","1~","1~","1~","","1~"]
["","Nome","","","","V1","V1","V1","","V1"]
["","Frequência","","","Hz","50","50","50","","50"]
["","Tensão","","","V","220-240","220-240","220-240","","220-240"]
["Potência nominal","Arrefecimento","","Nom.","kW","","","","0.028"]
["","Aquecimento","","Nom.","kW","","","","0.036"]
["Envolvente","Cor","","","","","","","Branco"]
["Dimensões","Unidade","","Altura","mm","","","","295"]
["","","","Largura","mm","","","","798"]
["","","","Profundidade","mm","","","","189"]
["Peso","Unidade","","","kg","","","","11.50"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","","","","13.1"]
["","","","Médio","m³/min","","","","9.8"]
["","","","B","m³/min","","","","7.2"]
["","","","Funcionamento silencioso","m³/min","","","","4.6"]
["","","Aquecimento","Alto","m³/min","","","","14.6"]
["","","","Médio","m³/min","","","","10.5"]
["","","","B","m³/min","","","","7.7"]
["","","","Funcionamento silencioso","m³/min","","","","5.2"]
["Nível de potência sonora","Arrefecimento","","","dBA","","","","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","","","45"]
["","","","Médio","dBA","","","","37"]
["","","","B","dBA","","","","29"]
["","","","Funcionamento silencioso","dBA","","","","21"]
["","Aquecimento","","Alto","dBA","","","","45"]
["","","","Médio","dBA","","","","37"]
["","","","B","dBA","","","","29"]
["","","","Funcionamento silencioso","dBA","","","","21"]
["Fluido frigorigéneo","GWP","","","","","","","675.0"]
["Ligações de tubagem","Líquido","","DE","mm","","","","6.35"]
["","Gás","","DE","mm","","","","12.70"]
["","Esgoto","","","","","","","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","","","","ARC466A58"]
["","Controlo remoto por cabo","","","","","","","BRC073"]
["Acessórios standard","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Filtro de ar","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Alimentação elétrica","Nome","","","","","","","V1"]
["","Fase","","","","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","","","50"]
["","Tensão","","","V","","","","220-240"]