{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BW","FTXA25C2V1BW","FTXA35C2V1BW","FTXA42C2V1BW","FTXA50C2V1BW"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.02","0.022","0.023","0.028","0.030"]
["","Aquecimento","","Nom.","kW","0.02","0.02","0.22","0.036","0.039"]
["Envolvente","Cor","","","","Branco","Branco","Branco","Branco","Branco"]
["Dimensões","Unidade","","Altura","mm","295","295","295","295","295"]
["","","","Largura","mm","798","798","798","798","798"]
["","","","Profundidade","mm","189","189","189","189","189"]
["Peso","Unidade","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","11","11.5","11.9","13.1","13.5"]
["","","","Médio","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","B","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Funcionamento silencioso","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Aquecimento","Alto","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","","Médio","m³/min","8.7","9","9","10.5","11.1"]
["","","","B","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Funcionamento silencioso","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Nível de potência sonora","Arrefecimento","","","dBA","57","57","60","60","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","39","40","41","45","46"]
["","","","Médio","dBA","32","33","33","37","39"]
["","","","B","dBA","25","25","25","29","31"]
["","","","Funcionamento silencioso","dBA","19","19","19","21","24"]
["","Aquecimento","","Alto","dBA","39","40","41","45","46"]
["","","","Médio","dBA","32","33","33","37","42"]
["","","","B","dBA","25","25","25","29","33"]
["","","","Funcionamento silencioso","dBA","19","19","19","21","24"]
["Fluido frigorigéneo","GWP","","","","675","675","675","675","675.0"]
["Ligações de tubagem","Líquido","","DE","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gás","","DE","mm","9.5","9.5","9.5","9.5","12.70"]
["","Esgoto","","","","18","18","18","18","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Controlo remoto por cabo","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Acessórios standard","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Filtro de ar","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Alimentação elétrica","Nome","","","","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240","220-240"]