{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B / 2MXF-A"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B / FTXF20B5V1B / 2MXF40A2V1B","FTXF25B5V1B / FTXF25B5V1B / 2MXF50A2V1B"]
["Capacidade de arrefecimento","Mín.","","kW","1.50","1.80"]
["","Máx.","","kW","4.20","5.30"]
["","Nom.","","kW","4.00","5.00"]
["Eficiência nominal","Annual energy consumption","","kWh","513","742"]
["","EER","","","3.90","3.37"]
["","COP","","","4.10","3.71"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A"]
["","","Aquecimento","","A","A"]
["Capacidade de aquecimento","Nom.","","kW","4.20","5.60"]
["","Mín.","","kW","1.30","1.20"]
["","Máx.","","kW","4.60","5.80"]