{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Nível de pressão sonora","Aquecimento","Alto","dBA","39","40"]
["","","Médio","dBA","34","34"]
["","","Funcionamento silencioso","dBA","21","21"]
["","","B","dBA","28","28"]
["","Arrefecimento","Medium","dBA","33","33"]
["","","Funcionamento silencioso","dBA","20","20"]
["","","B","dBA","25","26"]
["","","Alto","dBA","39","40"]
["Acessórios standard","Manual de instalação","","","1","1"]
["","Manual de funcionamento","","","1","1"]
["","Controle remoto por infravermelhos","","","1","1"]
["","Pilhas secas AAA","","","2","2"]
["","Suporte do controle remoto","","","1","1"]
["","Chapa de montagem","","","1","1"]
["","Parafusos de fixação da unidade interior","","","2","2"]
["Sistemas de controlo","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Controlo remoto por infravermelhos","","","ARC470A1","ARC470A1"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gás","DE","mm","9.50","9.50"]
["","Esgoto","","","18","18"]
["Potência absorvida","Arrefecimento","Nom.","kW","0.017","0.019"]
["","Aquecimento","Nom.","kW","0.020","0.020"]
["Nível de potência sonora","Arrefecimento","","dBA","55","55"]
["","Aquecimento","","dBA","55","55"]
["Dimensões","Unidade","Largura","mm","770","770"]
["","","Profundidade","mm","225","225"]
["","","Altura","mm","286","286"]
["Envolvente","Colour","","","Branco","Branco"]
["Peso","Unidade","","kg","8.50","8.50"]
["Power supply","Phase","","","1~","1~"]
["","Frequência","","Hz","50","50"]
["","Tensão","","V","220-240","220-240"]