{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Capacidade de arrefecimento","Nom.","","kW","4.00","4.00","4.00","5.20","6.00","4.00"]
["Eficiência nominal","Consumo anual de energia","","kWh","482","467","471","593","787","457"]
["","EER","","","4.15","4.28","4.25","4.38","3.81","4.38"]
["","COP","","","3.95","4.32","4.05","4.42","3.88","4.04"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A","A","A","A","A"]
["","","Aquecimento","","A","A","A","A","A","A"]
["Capacidade de aquecimento","Nom.","","kW","4.60","4.60","6.80","6.80","7.80","6.50"]
["Notas","","","","(1) - As capacidades de arrefecimento nominais são baseadas em: temp. interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m."]
["","","","","(2) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m."]
["","","","","(3) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","(4) - Consulte o esquema separado para conhecer os dados eléctricos"]