{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-K"]
[]
[]
[]
[]
["","","","","FTXM20K3V1B (Archived)","FTXM25K3V1B (Archived)","FTXM35K3V1B (Archived)","FTXM42K3V1B (Archived)","FTXM50K3V1B (Archived)"]
["Nível de pressão sonora","Aquecimento","Alto","dBA","40","41","45","45","47"]
["","","Funcionamento silencioso","dBA","19","19","19","22","24"]
["","","B","dBA","27","27","29","33","34"]
["","Arrefecimento","Funcionamento silencioso","dBA","19","19","19","21","23"]
["","","B","dBA","24","25","29","33","34"]
["","","Alto","dBA","40","41","45","45","46"]
["","","Nom.","dBA","34","34","39","39","40"]
["","Arrefecimento","Nom.","dBA","32","33","37","39","40"]
["Acessórios standard","Manual de funcionamento","","","1","1","1","1","1"]
["","Manual de instalação","","","1","1","1","1","1"]
["","Controle remoto por infravermelhos","","","1","1","1","1","1"]
["","Pilhas","","","2","2","2","2","2"]
["","Chapa de montagem","","","1","1","1","1","1"]
["","Parafusos de fixação da unidade interior","","","2","2","2","2","2"]
["","Filtro fotocatalítico de apatite de titânio","","","2","2","2","2","2"]
["","Suporte do controle remoto","","","1","1","1","1","1"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","ARC466A6","ARC466A6","ARC466A9","ARC466A9","ARC466A9"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gás","OD","mm","9.5","9.5","9.5","12.7","12.7"]
["","Drain","","","18","18","18","18","18"]
["Nível de potência sonora","Arrefecimento","","dBA","56","57","59","59","60"]
["","Aquecimento","","dBA","56","57","59","59","60"]
["Dimensões","Unidade","Width","mm","780","780","900","900","900"]
["","","Depth","mm","215","215","215","215","215"]
["","","Altura","mm","289","289","298","298","298"]
["Envolvente","Cor","","","Branco","Branco","Branco","Branco","Branco"]
["Peso","Unidade","","kg","8","8","11","11","11"]
["Power supply","Fase","","","1~","1~","1~","1~","1~"]
["","Frequência","","Hz","50","50","50","50","50"]
["","Nome","","","V1","V1","V1","V1","V1"]
["","Tensão","","V","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]