{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-N"]
[]
[]
[]
[]
["","","","","FTXM71R2V1B / RXM71N2V1B"]
["Capacidade de arrefecimento","Mín.","","kW","2.30"]
["","Máx.","","kW","8.50"]
["","Nom.","","kW","7.10"]
["Eficiência nominal","Consumo anual de energia","","kWh","1,172"]
["","EER","","","3.03"]
["","COP","","","3.19"]
["","Diretiva de etiqueta da energia","Arrefecimento","","B"]
["","","Aquecimento","","D"]
["Capacidade de aquecimento","Nom.","","kW","8.20"]
["","Mín.","","kW","2.30"]
["","Máx.","","kW","10.20"]
["Notas","","","","(1) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","(2) - Consulte o esquema separado para conhecer os dados eléctricos"]
["","","","","(3) - As capacidades de arrefecimento nominais são baseadas em: temp. interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m."]
["","","","","(4) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m."]