{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Outdoor unit","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Capacidade de arrefecimento","Mín.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Máx.","","kW","","3.0"]
["Capacidade de aquecimento","Mín.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Máx.","","kW","","4.00"]
["Eficiência nominal","Consumo anual de energia","","kWh","","326"]
["","COP","","","","4.36"]
["","EER","","","","3.83"]
["","Diretiva de etiqueta da energia","Arrefecimento","","","A"]
["","","Aquecimento","","","A"]
["Notas","","","","","(1) - As capacidades de arrefecimento nominais são baseadas em: temperatura interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m."]
["","","","","","(2) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m."]
["","","","","","(3) - Consulte o esquema separado para conhecer os dados eléctricos"]
["Capacidade de arrefecimento","Mín.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Máx.","","kW","2.6","","4.0"]
["Capacidade de aquecimento","Mín.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Máx.","","kW","3.50","","4.80"]
["Eficiência nominal","EER","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Consumo anual de energia","","kWh","249"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","","A"]
["","","Aquecimento","","A","","A"]
["Arrefecimento ambiente","Classe de eficiência energética","","","A++","","A++"]
["","Capacidade","Pdesign","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Consumo anual de energia","","kWh/a","103","","186"]
["Aquecimento ambiente (clima médio)","Classe de eficiência energética","","","A++","","A++"]
["","Capacidade","Pdesign","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Capacidade de aquecimento Pdh a -10°","","kW","1.99","","2.33"]
["","Consumo anual de energia","","kWh/a","662","","845"]
["Gama de eficiência energética","","","","A+++ ~ D","","A+++ ~ D"]