{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","40","","","","","","45"]
["","","","Funcionamento silencioso","dBA","19","","","","","","22"]
["","","","B","dBA","27","","","","","","33"]
["","Arrefecimento","","Funcionamento silencioso","dBA","19","","","","","","21"]
["","","","B","dBA","24","","","","","","33"]
["","","","Alto","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Arrefecimento","","Nom.","dBA","32","","","","","","39"]
["Acessórios standard","Manual de instalação","","","","1","","","","","","1"]
["","Manual de funcionamento","","","","1","","","","","","1"]
["","Controle remoto sem fios","","","","1","","","","","","1"]
["","Pilhas","","","","2","","","","","","2"]
["","Suporte do controle remoto","","","","1","","","","","","1"]
["","Chapa de montagem","","","","1","","","","","","1"]
["","Filtro fotocatalítico de apatite de titânio","","","","2","","","","","","2"]
["","Parafusos de fixação da unidade interior","","","","2","","","","","","2"]
["Sistemas de controlo","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Ligações de tubagens","Liquid","","OD","mm","6.35","","","","","","6.35"]
["","Gás","","OD","mm","9.5","","","","","","9.5"]
["","Drain","","","","18","","","","","","18"]
["Power input","Arrefecimento","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Aquecimento","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Arrefecimento","","","dBA","58","","","","","","59"]
["","Aquecimento","","","dBA","58","","","","","","59"]
["Dimensões","Unidade","","Largura","mm","780","","","","","","900"]
["","","","Profundidade","mm","215","","","","","","215"]
["","","","Altura","mm","289","","","","","","298"]
["Envolvente","Cor","","","","Branco","","","","","","Branco"]
["Peso","Unidade","","","kg","8","","","","","","11"]
["Power supply","Fase","","","","1~","","","","","","1~"]
["","Frequência","","","Hz","50","","","","","","50"]
["","Nome","","","","V1","","","","","","V1"]
["","Tensão","","","V","220-240","","","","","","220-240"]
["Notas","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Quando ligado com unidade exterior de multi-sistema, consulte as especificações da unidade exterior multi a ser ligada.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","","","","","(4) - 240V"]
["Potência nominal","Arrefecimento","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Aquecimento","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Envolvente","Cor","","","","","Branco","Branco","Branco","Branco","Branco","","Branco","Branco","Branco"]
["Dimensões","Unidade","","Altura","mm","","215","289","215","298","215","","215","298","215"]
["","","","Largura","mm","","780","780","780","900","900","","900","900","900"]
["","","","Profundidade","mm","","289","215","289","215","298","","298","215","298"]
["Peso","Unidade","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Médio","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","B","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Funcionamento silencioso","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Aquecimento","Alto","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Médio","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","B","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Funcionamento silencioso","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Nível de potência sonora","Arrefecimento","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Aquecimento","","","dBA","","58","58","58","59","59","","59","60","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Médio","dBA","","32","33","33","","37","","39","","40"]
["","","","B","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Funcionamento silencioso","dBA","","19","19","19","19","19","","21","23","23"]
["","Aquecimento","","Alto","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Médio","dBA","","34","34","34","","39","","39","","40"]
["","","","B","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Funcionamento silencioso","dBA","","19","19","19","19","19","","22","24","24"]
["Ligações de tubagem","Líquido","","DE","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gás","","DE","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Esgoto","","","","","18","18","18","18","18","","18","18","18"]
["Sistemas de controlo","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Acessórios standard","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Alimentação elétrica","Nome","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Tensão","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilador","Caudal de ar","Arrefecimento","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilador","Caudal de ar","Aquecimento","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Nível de pressão sonora","Aquecimento","","Nom.","dBA","","","34","","39","","","","40"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Acessórios standard","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]