{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTJ-AB"]
[]
[]
[]
[]
["","","","","","FTXTJ30A2V1BB"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.024"]
["","Aquecimento","","Nom.","kW","0.024"]
["Envolvente","Cor","","","","Preto"]
["Dimensões","Unidade","","Altura","mm","305"]
["","","","Largura","mm","900"]
["","","","Profundidade","mm","212"]
["Peso","Unidade","","","kg","12"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","12.1"]
["","","","Médio","m³/min","8.8"]
["","","","B","m³/min","5.9"]
["","","","Funcionamento silencioso","m³/min","4.9"]
["","","Aquecimento","Alto","m³/min","12.3"]
["","","","Médio","m³/min","7.8"]
["","","","B","m³/min","6.5"]
["","","","Funcionamento silencioso","m³/min","4.5"]
["Nível de potência sonora","Arrefecimento","","","dBA","60"]
["","Aquecimento","","","dBA","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","43"]
["","","","Médio","dBA","32"]
["","","","B","dBA","25"]
["","","","Funcionamento silencioso","dBA","20"]
["","Aquecimento","","Alto","dBA","41"]
["","","","Médio","dBA","31"]
["","","","B","dBA","24"]
["","","","Funcionamento silencioso","dBA","19"]
["Fluido frigorigéneo","GWP","","","","675"]
["Ligações de tubagem","Líquido","","DE","mm","6.35"]
["","Gás","","DE","mm","9.5"]
["","Esgoto","","","","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC488A4K"]
["Sistemas de controlo","Controlo remoto por cabo","","","","BRC073A1"]
["Acessórios standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]