{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.029","0.053"]
["","Aquecimento","","Nom.","kW","0.024","0.06"]
["Envolvente","Cor","","","","Branco","Branco"]
["Dimensões","Unidade","","Altura","mm","298","298"]
["","","","Largura","mm","804","997"]
["","","","Profundidade","mm","252","292"]
["Peso","Unidade","","","kg","12","15"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","13.2","15.1"]
["","","","Médio","m³/min","8.1","9.2"]
["","","","B","m³/min","5.6","5.6"]
["","","","Funcionamento silencioso","m³/min","4.8","4.8"]
["","","Aquecimento","Alto","m³/min","11.7","17"]
["","","","Médio","m³/min","7.7","10"]
["","","","B","m³/min","5.6","6"]
["","","","Funcionamento silencioso","m³/min","4.7","5.1"]
["Nível de potência sonora","Arrefecimento","","","dBA","60","60"]
["","Aquecimento","","","dBA","59","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","45","46"]
["","","","Médio","dBA","33","32"]
["","","","B","dBA","25","24"]
["","","","Funcionamento silencioso","dBA","21","20"]
["","Aquecimento","","Alto","dBA","43","46"]
["","","","Médio","dBA","31","31"]
["","","","B","dBA","22","22"]
["","","","Funcionamento silencioso","dBA","19","19"]
["Fluido frigorigéneo","GWP","","","","675","675"]
["Ligações de tubagem","Líquido","","DE","mm","6.35","6.35"]
["","Gás","","DE","mm","9.5","9.5"]
["","Esgoto","","","","18","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A83","ARC466A83"]
["Acessórios standard","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentação elétrica","Nome","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]
["Notas","","","","","(1) - Arrefecimento: temp. interior: 27°CBs, 19°CBh; temp. exterior 35°CBs; 24°CBh; comprimento equivalente de tubagem: 5m","(1) - Arrefecimento: temp. interior: 27°CBs, 19°CBh; temp. exterior 35°CBs; 24°CBh; comprimento equivalente de tubagem: 5m"]
["","","","","","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 5m","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 5m"]
["","","","","","(3) - Consulte o esquema separado para conhecer os dados eléctricos","(3) - Consulte o esquema separado para conhecer os dados eléctricos"]
["Acessórios standard","FTXTM40A2V1B","","","","","1"]