{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","","","","41","46","47"]
["","","","Médio","dBA","","","","38","42","43"]
["","","","B","dBA","","","","35","39","40"]
["","Arrefecimento","","Médio","dBA","","","","38","42","43"]
["","","","B","dBA","","","","35","39","40"]
["","","","Alto","dBA","","","","41","46","47"]
["Acessórios standard","Manual de funcionamento","","","","","","","1","1","1"]
["","Manual de instalação","","","","","","","1","1","1"]
["","Tubo flexível de drenagem","","","","","","","1","1","1"]
["","Tubo de isolamento térmico","","","","","","","3","3","3"]
["","Atilhos","","","","","","","10","10","10"]
["","Braçadeira do tubo flexível","","","","","","","1","1","1"]
["","Material vedante","","","","","","","4","4","4"]
["","Chapa de fixação da anilha","","","","","","","1","1","1"]
["","União de drenagem","","","","","","","1","1","1"]
["","Tecido não entrelaçado","","","","","","","1","1","1"]
["","Anilha","","","","","","","8","8","8"]
["","Parafuso de fixação para tubo flexível de drenagem","","","","","","","5","5","5"]
["Sistemas de controlo","Controlo remoto por cabo","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Capacidade de arrefecimento","Capacidade total","","Nom.","kW","","","","","","12.1"]
["Piping connections","Líquido","","DE","mm","","","","9.52","9.52","9.52"]
["","Gás","","DE","mm","","","","15.9","15.9","15.9"]
["","Esgoto","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Nível de potência sonora","Arrefecimento","","","dBA","","","","59","64","65"]
["","Aquecimento","","","dBA","","","","59","64"]
["Dimensões","Unidade","","Largura","mm","","","","950","950","950"]
["","","","Profundidade","mm","","","","950","950","950"]
["","","","Altura","mm","","","","198","198","198"]
["Casing","Material","","","","","","","Resina","Resina","Resina"]
["","Colour","","","","","","","Branco fresco","Branco fresco","Branco fresco"]
["Peso","Unidade","","","kg","","","","25.0","26.0","26"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","","","","23.0","31.0","32.5"]
["","","","Médio","m³/min","","","","19.5","25.5","26.5"]
["","","","B","m³/min","","","","16.0","20.0","20.5"]
["","","Arrefecimento","B","m³/min","","","","16.0","20.0","20.5"]
["","","","Médio","m³/min","","","","19.5","25.5","26.5"]
["","","","Alto","m³/min","","","","23.0","31.0","32.5"]
["Altura de drenagem","mm","","","","","","","600","600","600"]
["Capacidade de aquecimento","Capacidade total","","Nom.","kW","","","","","","13.5"]
["Envolvente","Cor","","","","Branco fresco","Branco fresco","Branco fresco"]
["","Material","","","","Resina","Resina","Resina"]
["Dimensões","Unidade","","Altura","mm","198","198","198"]
["","","","Largura","mm","950","950","950"]
["","","","Profundidade","mm","950","950","950"]
["Peso","Unidade","","","kg","25.0","26.0","26.0"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","23.0","31.0","32.5"]
["","","","Médio","m³/min","19.5","25.5","26.5"]
["","","","B","m³/min","16.0","20.0","20.5"]
["","","Aquecimento","Alto","m³/min","23.0","31.0","32.5"]
["","","","Médio","m³/min","19.5","25.5","26.5"]
["","","","B","m³/min","16.0","20.0","20.5"]
["Nível de potência sonora","Arrefecimento","","","dBA","59","64","65"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","41","46","47"]
["","","","Médio","dBA","38","42","43"]
["","","","B","dBA","35","39","40"]
["","Aquecimento","","Alto","dBA","41","46","47"]
["","","","Médio","dBA","38","42","43"]
["","","","B","dBA","35","39","40"]
["Ligações de tubagem","Líquido","","DE","mm","9.52","9.52","9.52"]
["","Gás","","DE","mm","15.9","15.9","15.9"]
["","Esgoto","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Altura de drenagem","mm","","","","600","600","600"]
["Acessórios standard","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Capacidade de arrefecimento","Capacidade total","","Nom.","kW","","","12.10"]
["Capacidade de aquecimento","Capacidade total","","Nom.","kW","","","13.5"]