{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L8Y1B","FUQ71CVEB / RZQG71L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG100L8Y1B","FUQ100CVEB / RZQG100L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG125L8Y1B","FUQ125CVEB / RZQG125L8Y1B"]
["Capacidade de arrefecimento","Nom.","","kW","","6.8","","9.5","","12.0"]
["Arrefecimento ambiente","SEER","","","6.50","6.42","5.10","6.11","5.10","5.61"]
["","Consumo anual de energia","","kWh/a","367","371","652","545","824","749"]
["","Capacidade","Pdesign","kW","6.80","6.80","9.50","9.5","12.00","12"]
["","Classe de eficiência energética","","","A++","A++","B","A++","B","A+"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","7.60","7.60","11.30","11.3","12.71","14.13"]
["","SCOP/A","","","4.20","4.20","3.80","4.5","3.80","4.44"]
["","Classe de eficiência energética","","","A+","A+","A","A+","A","A+"]
["","Consumo anual de energia","","kWh/a","2,534","2,534","4,164","3,516","4,683","4,456"]
["Eficiência nominal","Annual energy consumption","","kWh","","840","","1,230","","1,770"]
["","EER","","","","4.05","","3.86","","3.39"]
["","COP","","","","4.08","","3.95","","3.42"]
["","Diretiva de etiqueta da energia","Arrefecimento","","","A","","A","","A"]
["","","Aquecimento","","","A","","A","","B"]
["Capacidade de aquecimento","Nom.","","kW","","7.5","","10.8","","13.5"]
["Notas","","","","","(1) - Consumo anual de energia de acordo com a directiva de etiquetagem de energia 2002/31/EC","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","","(2) - SEER e SCOP de acordo com a EN 14825","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]