{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L8Y1B","FVQ100CVEB / RZQG71L8Y1B","FVQ140CVEB / RZQG100L8Y1B","FVQ125CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG140L7Y1B"]
["Capacidade de arrefecimento","Nom.","","kW","6.8","","","12.0","","13.4"]
["Arrefecimento ambiente","SEER","","","6.23","6.31","5.61","5.61","5.61"]
["","Consumo anual de energia","","kWh/a","383","378","593","748.663","749"]
["","Capacidade","Pdesign","kW","6.80","6.80","9.50","12.00","12.00"]
["","Classe de eficiência energética","","","A++","A++","A+","A+","A+"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","6.33","6.33","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","3.87","3.87"]
["","Classe de eficiência energética","","","A+","A+","A+","A","A"]
["","Consumo anual de energia","","kWh/a","2,189","2,189","3,767","4,087.855","4,088"]
["Eficiência nominal","Consumo anual de energia","","kWh","1,010","","","1,870","","2,085"]
["","EER","","","3.37","","","3.21","","3.21"]
["","COP","","","3.64","","","3.70","","3.61"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","","","A"]
["","","Aquecimento","","A","","","A"]
["Capacidade de aquecimento","Nom.","","kW","7.5","","","13.5","","15.5"]
["Notas","","","","(1) - Consumo anual de energia de acordo com a directiva de etiquetagem de energia 2002/31/EC","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - SEER e SCOP de acordo com a EN 14825","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]