{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Capacidade de arrefecimento","Mín.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","2.5","3.5","5.0"]
["","Máx.","","kW","3.0","3.8","5.6"]
["Capacidade de aquecimento","Mín.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","3.4","4.5","5.8"]
["","Máx.","","kW","4.5","5.0","8.1"]
["Eficiência nominal","EER","","","4.63","3.72","3.31"]
["","COP","","","4.42","3.75","3.69"]
["","Consumo anual de energia","","kWh","270","470","755"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A","A"]
["","","Aquecimento","","A","A","A"]
["Ligações de tubagem","Gás","DE","mm","9.5","9.5","12.7"]
["","Líquido","DE","mm","6.35","6.35","6.35"]
["Arrefecimento ambiente","Classe de eficiência energética","","","A++","A++","A"]
["","Capacidade","Pdesign","kW","2.50","3.50","5.00"]
["","SEER","","","6.53","6.48","5.41"]
["","Consumo anual de energia","","kWh/a","134","189","324"]
["Aquecimento ambiente (clima médio)","Classe de eficiência energética","","","A++","A+","A+"]
["","Capacidade","Pdesign","kW","2.80","3.10","4.60"]
["","SCOP/A","","","4.65","4.00","4.18"]
["","Consumo anual de energia","","kWh/a","842","1087","1543"]
["Notas","","","","(1) - Arrefecimento: temp. interior 27 °CBs, 19 °CBh; temp. exterior 35 °CBs, 24 °CBh","(1) - Arrefecimento: temp. interior 27 °CBs, 19 °CBh; temp. exterior 35 °CBs, 24 °CBh","(1) - Arrefecimento: temp. interior 27 °CBs, 19 °CBh; temp. exterior 35 °CBs, 24 °CBh"]
["","","","","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh"]