{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":11,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXT-ATV3"]
[]
[]
[]
[]
["","","","","","FWXT10ABTV3","FWXT15ABTV3","FWXT20ABTV3","FWXT10AATV3 (Archived)","FWXT15AATV3 (Archived)","FWXT20AATV3 (Archived)"]
["Dimensões","Unidade","","Width","mm","","","","902","1,100","1,300"]
["","","","Depth","mm","","","","128","128","128"]
["","","","Altura","mm","","","","335","335","335"]
["Envolvente","Cor","","","","","","","RAL 9003","RAL 9003","RAL 9003"]
["Peso","Unidade","","","kg","","","","14.0","16.0","19.0"]
["Power supply","Fase","","","","","","","1~","1~","1~"]
["","Frequência","","","Hz","","","","50","50","50"]
["","Tensão","","","V","","","","230","230","230"]
["Capacidade de arrefecimento","7/12 °C","","Mín.","kW","0.49","0.62","0.70"]
["","","","Méd.","kW","0.88","1.08","1.21"]
["","","","Máx.","kW","1.24","1.61","1.94"]
["Capacidade de arrefecimento sensível","7/12 °C","","Mín.","kW","0.37","0.52","0.57"]
["","","","Méd.","kW","0.70","0.86","1.02"]
["","","","Máx.","kW","0.98","1.27","1.52"]
["Capacidade de aquecimento","45/40 °C","","Mín.","kW","0.55","0.79","0.74"]
["","","","Capacidade de aquecimento-=-45/40 °C-=-Méd.-=-kW","kW","1.00","1.36","1.55"]
["","","","Máx.","kW","1.50","2.01","2.13"]
["Potência absorvida","Mín.","","","kW","0.01","0.01","0.01"]
["","Méd.","","","kW","0.01","0.01","0.01"]
["","Máx.","","","kW","0.02","0.02","0.03"]
["Velocidade do ventilador","Mín.","","","rpm","680.00","680.00","680.00"]
["","Méd.","","","rpm","1100.00","1100.00","1100.00"]
["","Velocidade do ventilador-=-Máx.-=-rpm","","","rpm","1500.00","1500.00","1500.00"]
["Envolvente","Cor","","","","RAL 9003","RAL 9003","RAL 9003"]
["","Material","","","","Folha de metal","Folha de metal","Folha de metal"]
["Dimensões","Unidade","","Altura","mm","335","335","335"]
["","","","Largura","mm","902","1102","1302"]
["","","","Profundidade","mm","128","128","128"]
["","Unidade embalada","","Altura","mm","490","490","490"]
["","","","Largura","mm","1030","1230","1430"]
["","","","Profundidade","mm","210","210","210"]
["Peso","Unidade","","","kg","14","16","19"]
["","Unidade embalada","","","kg","15","17","20"]
["Acondicionamento","Material","","","","Cartão","Cartão","Cartão"]
["","Peso","","","kg","1","1","1"]
["Permutador de calor","Quantidade","","","","1","1","1"]
["","Volume da serpentina interna","","","l","0.5","0.61","0.77"]
["","Carregamento","","Pressão de funcionamento","bar","10","10","10"]
["Circuito de água","Diâmetro das ligações de tubagens","","","inch","3/4","3/4","3/4"]
["","Material da tubagem","","","","COBRE","COBRE","COBRE"]
["","Pressão","Aquecimento","Máx.","bar","10","10","10"]
["Circuito de água - queda de pressão da água","Aquecimento","45/40 °C","Mín.","kPa","5.10","4.81","6.00"]
["","","","Méd.","kPa","12.00","6.30","6.40"]
["","","","Máx.","kPa","16.30","7.20","8.10"]
["","Arrefecimento","7/12 °C","Mín.","kPa","4.80","4.70","5.50"]
["","","","Méd.","kPa","10.50","5.60","5.40"]
["","","","Máx.","kPa","11.70","5.10","5.30"]
["Circuito de água - caudal de água","Aquecimento","45/40 °C","Mín.","kg/h","100.00","140","150.00"]
["","","","Méd.","kg/h","170.00","240","300.00"]
["","","","Máx.","kg/h","260.00","350","420.00"]
["","Arrefecimento","7/12 °C","Mín.","kg/h","80.00","110","120.00"]
["","","","Méd.","kg/h","150.00","190","210.00"]
["","","","Máx.","kg/h","210.00","280","330.00"]
["Nível de potência sonora","Mín.","","","dBA","35","36","37"]
["","Méd.","","","dBA","46","47","48"]
["","Máx.","","","dBA","53.0","54.0","55.0"]
["Limite de funcionamento","Aquecimento","Lado da água","Mín.","°C","30","30","30"]
["","","","Máx.","°C","85","85","85"]
["","Arrefecimento","Lado da água","Mín.","°C","5","5","5"]
["","","","Máx.","°C","18","18","18"]
["","Instalação no interior","Ambiente","Mín.","° CBs","0","0","0"]
["","","","Máx.","° CBs","45","45","45"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","Para FWXT-ATV3(C)(CL)","Para FWXT-ATV3(C)(CL)","Para FWXT-ATV3(C)(CL)"]
["","Incorporado na unidade interior","","","","Sim","Sim","Sim"]
["Alimentação elétrica","Fase","","","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","230","230","230"]
["Consumo de energia eléctrica","Máx.","","","W","19","20","29"]
["","Standby","","","W","3","4","5"]
["Corrente","Corrente de funcionamento máxima","","Aquecimento","A","0.16","0.18","0.24"]
["","Corrente máxima de funcionamento","","Arrefecimento","A","0.16","0.18","0.24"]