{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRLEQ-BY1"]
[]
[]
[]
[]
["","","","","","LRLEQ3BY1","LRLEQ4BY1"]
["Acessórios standard","Manual de instalação","","","","1","1"]
["","Precauções gerais de segurança","","","","1","1"]
["Capacidade de refrigeração","Baixa temperatura","","kW","kW","2.78 (1)","3.62 (1)"]
["Peso","Unidade","","","kg","130","130"]
["Fluido frigorigéneo","Charge","","","TCO2Eq","14.4","14.4"]
["","GWP","","","","2,087.5","2,087.5"]
["","Carga","","","kg","6.90","6.90"]
["","Type","","","","R-410A","R-410A"]
["Motor do ventilador","Potência absorvida","","","W","70","70"]
["","Acionamento","","","","Accionamento directo","Accionamento directo"]
["Permutador de calor","Type","","","","Serpentina de alheta transversal","Serpentina de alheta transversal"]
["Power input","Baixa temperatura","","Nom.","kW","2.60 (1)","3.41 (1)"]
["COP","Low temperature","","Nom.","","1.07 (1)","1.06 (1)"]
["Dimensões","Unidade","","Width","mm","900","900"]
["","","","Depth","mm","320","320"]
["","","","Altura","mm","1,345","1,345"]
["Envolvente","Cor","","","","Branco Daikin","Branco Daikin"]
["Ventilador","Tipo","","","","Hélice","Hélice"]
["","Caudal de ar","Arrefecimento","Nom.","m³/min","106","106"]
["","Quantidade","","","","2","2"]
["Power supply","Fase","","","","3N~","3N~"]
["","Frequência","","","Hz","50","50"]
["","Tensão","","","V","380-415","380-415"]
["Notas","","","","","(1) - Arrefecimento: temp. de evaporação -35℃; temp. exterior 32°C; aspiração SH10°C","(1) - Arrefecimento: temp. de evaporação -35℃; temp. exterior 32°C; aspiração SH10°C"]
["","","","","","(2) - Dados de pressão sonora: medidos a 1 m em frente à unidade, a 1,5 m de altura","(2) - Dados de pressão sonora: medidos a 1 m em frente à unidade, a 1,5 m de altura"]