{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-E"]
[]
[]
[]
[]
["","","","","","RXF20E5V1B","RXF25E5V1B","RXF35E5V1B","RXF42E5V1B"]
["Dimensões","Unidade","","Altura","mm","556","556","556","556"]
["","","","Largura","mm","740","740","740","740"]
["","","","Profundidade","mm","343","343","343","343"]
["Peso","Unidade","","","kg","24.0","24.0","24.0","28.0"]
["Compressor","Tipo","","","","Compressor oscilante hermético","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","-10","-10","-10","-10"]
["","","","Máx.","°CBs","48","48","48","48"]
["","Aquecimento","Ambiente","Mín.","°CWB","-15","-15","-15","-15"]
["","","","Máx.","°CWB","18","18","18","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","46.0","46.0","48.0","48.0"]
["","Aquecimento","","Alto","dBA","47.0","47.0","48.0","48.0"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.420","0.420","0.550","0.750"]
["","Carga","","","tCO2Eq","0.280","0.280","0.370","0.510"]
["","GWP","","","","675.0","675.0","675.0","675.0"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20","20","20","20"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","12.0","12.0","12.0","12.0"]
["Acessórios standard","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240"]
["Compressor","Tipo","","","","","Compressor oscilante hermético"]