{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","","47","48"]
["","Arrefecimento","","Alto","dBA","","46","48"]
["Acessórios standard","Junta (drenagem)","","","","","1","1"]
["","Manual de instalação","","","","","1","1"]
["Fluido frigorigéneo","Charge","","","TCO2Eq","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","1.05","1.05"]
["","Tipo","","","","","R-410A","R-410A"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","","780","780"]
["","","Aquecimento","Super baixa","rpm","","740","740"]
["Ligações de tubagens","Diferença de nível","IU - OU","Máx.","m","","15","15"]
["","Carga de refrigerante adicional","","","kg/m","","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["Compressor","Tipo","","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Dimensões","Unidade","","Largura","mm","","765","765"]
["","","","Profundidade","mm","","285","285"]
["","","","Altura","mm","","550","550"]
["Peso","Unidade","","","kg","","35","35"]
["Ventilador","Caudal de ar","Aquecimento","Super baixa","cfm","","932","932"]
["","","Arrefecimento","Super baixa","cfm","","1,094","1,094"]
["Power supply","Fase","","","","","1~","1~"]
["","Frequência","","","Hz","","50","50"]
["","Tensão","","","V","","220-240","220-240"]
["Notas","","","","","(1) - 220V","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - Limites de funcionamento em combinação com a unidade Nexura, FVXG-K, arrefecimento: mín. 10°CBs - máx. 46°CBs; aquecimento: mín. -15°CBh - máx. 18°CBh","(4) - 240V","(4) - 240V","(4) - Limites de funcionamento em combinação com a unidade Nexura, FVXG-K, arrefecimento: mín. 10°CBs - máx. 46°CBs; aquecimento: mín. -15°CBh - máx. 18°CBh"]
["","","","","","","(5) - Limites de funcionamento em combinação com a unidade Nexura, FVXG-K, arrefecimento: mín. 10°CBs - máx. 46°CBs; aquecimento: mín. -15°CBh - máx. 18°CBh","(5) - Limites de funcionamento em combinação com a unidade Nexura, FVXG-K, arrefecimento: mín. 10°CBs - máx. 46°CBs; aquecimento: mín. -15°CBh - máx. 18°CBh"]
["","","","","","","(6) - Contém gases fluorados com efeito de estufa","(6) - Contém gases fluorados com efeito de estufa"]
["Ventilador","Caudal de ar","Arrefecimento","Super baixa","m³/min","31.0","","","42.6"]
["","","Aquecimento","Super baixa","m³/min","26.4","","","38.3"]
["","","","Super baixa","cfm","1094","","","1504"]
["","","Aquecimento","Super baixa","cfm","932","","","1352"]
["Dimensões","Unidade","","Altura","mm","550","","","735"]
["","","","Largura","mm","765","","","825"]
["","","","Profundidade","mm","285","","","300"]
["Peso","Unidade","","","kg","35","","","48"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","780","","","670"]
["","","Aquecimento","Super baixa","rpm","740","","","670"]
["Compressor","Tipo","","","","Compressor oscilante hermético","","","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10 (5)","","","-10 (5)"]
["","","","Máx.","° CBs","46","","","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15","","","-15"]
["","","","Máx.","° CBh","18","","","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","46","","","48"]
["","Aquecimento","","Alto","dBA","47","","","48"]
["Fluido frigorigéneo","Tipo","","","","R-410A","","","R-410A"]
["","Carga","","","kg","1.05","","","1.6"]
["","Carga","","","tCO2Eq","2.2","","","3.3"]
["","GWP","","","","2087.5","","","2087.5"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20","","","30"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","","","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","15","","","20"]
["Acessórios standard","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Alimentação elétrica","Fase","","","","1~","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","","","50"]
["","Tensão","","","V","220-240","","","220-240"]