{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M9"]
[]
[]
[]
[]
["","","","","","RXM20M3V1B9","RXM25M3V1B9","RXM35M3V1B9","RXM42M3V1B9 (Archived)","RXM50M3V1B9 (Archived)","RXM60M3V1B9 (Archived)"]
["Dimensões","Unidade","","Altura","mm","550","550","550","735","735","735"]
["","","","Largura","mm","765","765","765","825","825","825"]
["","","","Profundidade","mm","285","285","285","300","300","300"]
["Peso","Unidade","","","kg","32","32","32","47","47","47"]
["Compressor","Type","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","","","Compressor oscilante hermético"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","46","46","49","48","48","48"]
["","Aquecimento","","Nom.","dBA","47","47","49","48","49","49"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.76","0.76","0.76","1.30","1.40","1.45"]
["","Carga","","","tCO2Eq","0.52","0.52","0.52","0.88","0.95","0.98"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20.0","20.0","20.0","30","30","30"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","15.0","15.0","15.0","20","20","20"]
["Acessórios standard","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Compressor","Tipo","","","","","","","Compressor oscilante hermético","Compressor oscilante hermético"]