{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":11,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP71N5V1B9","RXP60N5V1B9 (Archived)"]
["Dimensões","Unidade","","Altura","mm","556","556","556","734","734","734"]
["","","","Largura","mm","740","740","740","954","954","954"]
["","","","Profundidade","mm","343","343","343","401","401","401"]
["Peso","Unidade","","","kg","24","24","26","46","50","50"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10","-10","-10"]
["","","","Máx.","° CBs","48","48","48"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15","-15","-15"]
["","","","Máx.","° CBh","18","18","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","46","46","48"]
["","","","Nom.","dBA","","","","47","52","49"]
["","Aquecimento","","Alto","dBA","47","47","48"]
["","","","Nom.","dBA","","","","49","52","49"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.55","0.55","0.70","0.9","1.15","1.15"]
["","Carga","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20","20","20","30","30","30"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","12","12","12","20","20","20"]
["Acessórios standard","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Compressor","Tipo","","","","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Acessórios standard","Drain cap","","","","","","","3","3","3"]
["Gama de eficiência energética","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notas","","","","","","","","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","","","","(2) - Consulte o esquema separado para conhecer os dados eléctricos","(2) - Consulte o esquema separado para conhecer os dados eléctricos","(2) - Consulte o esquema separado para conhecer os dados eléctricos"]
["","","","","","","","","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa"]