{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","49","","","52"]
["","","","B","dBA","46","","","49"]
["","Arrefecimento","","B","dBA","46","","","49"]
["","","","Alto","dBA","49","","","52"]
["Acessórios standard","Tomada de drenagem","","","","1","","","1"]
["","Manual de instalação","","","","1","","","1"]
["Fluido frigorigéneo","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Carga","","","kg","1.5","","","2.3"]
["","Tipo","","","","R-410A","","","R-410A"]
["Piping connections","Diferença de nível","IU - OU","Máx.","m","20","","","20"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","","","0,02 (para comprimento de tubagem superior a 10m)"]
["Nível de potência sonora","Arrefecimento","","","dBA","","","","65"]
["Compressor","Type","","","","Compressor oscilante hermético","","","Compressor oscilante hermético"]
["Dimensões","Unidade","","Largura","mm","825","","","900"]
["","","","Profundidade","mm","300","","","320"]
["","","","Altura","mm","735","","","770"]
["Peso","Unidade","","","kg","48","","","71"]
["Power supply","Fase","","","","1~","","","1~"]
["","Frequência","","","Hz","50","","","50"]
["","Tensão","","","V","220-240","","","220-240"]
["Notas","","","","","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - 220V","","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar","(1) - 220V"]
["","","","","","(2) - Contém gases fluorados com efeito de estufa","(2) - 230V","","(2) - Contém gases fluorados com efeito de estufa","(2) - 230V"]
["Dimensões","Unidade","","Altura","mm","","735","735","","770","770"]
["","","","Largura","mm","","825","825","","900","900"]
["","","","Profundidade","mm","","300","300","","320","320"]
["Peso","Unidade","","","kg","","48","48","","71","71"]
["Compressor","Type","","","","","Compressor oscilante hermético","Compressor oscilante hermético","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","","-10","-10","","-10","-10"]
["","","","Máx.","°CBs","","46","46","","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","","-15","-15","","-15","-15"]
["","","","Máx.","° CBh","","18","20","","18","20"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","49","49","","52","52"]
["","","","B","dBA","","46","46","","49","49"]
["","Aquecimento","","Alto","dBA","","49","49","","52","52"]
["","","","B","dBA","","46","46","","49","49"]
["Fluido frigorigéneo","Tipo","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Carga","","","kg","","1.5","1.5","","2.3","2.3"]
["","Carga","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","","30","30","","30","30"]
["","Carga de refrigerante adicional","","","kg/m","","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)","","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","","20","20","","20","20"]
["Acessórios standard","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Alimentação elétrica","Fase","","","","","1~","1~","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","50","50","","50","50"]
["","Tensão","","","V","","220-240","220-240","","220-240","220-240"]
["Notas","","","","","","(3) - 240V","","","(3) - 240V"]
["Acessórios standard","Drain socket","","","","","","1","","","1"]