{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilador","Caudal de ar","Arrefecimento","Super baixa","m³/min","46.0"]
["","","Aquecimento","Super baixa","m³/min","46.0"]
["","","","Super baixa","cfm","1624"]
["","","Aquecimento","Super baixa","cfm","1624"]
["Dimensões","Unidade","","Altura","mm","770"]
["","","","Largura","mm","900"]
["","","","Profundidade","mm","320"]
["Peso","Unidade","","","kg","71"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","730"]
["","","Aquecimento","Super baixa","rpm","730"]
["Compressor","Tipo","","","","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","-10"]
["","","","Máx.","°CBs","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15"]
["","","","Máx.","° CBh","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","52"]
["","Aquecimento","","Alto","dBA","52"]
["Fluido frigorigéneo","Tipo","","","","R-410A"]
["","Carga","","","kg","2.3"]
["","Carga","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","30"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","20"]
["Acessórios standard","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]
["Notas","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]