{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":11,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","47","47","48","48"]
["","Arrefecimento","","Alto","dBA","46","46","48","48"]
["Acessórios standard","Tampão de drenagem","","","","1","1","1","1"]
["","Manual de instalação","","","","1","1","1","1"]
["","Etiqueta da carga de refrigerante","","","","1","1","1"]
["","Etiquetas multilingues relativas aos gases de estufa fluorados","","","","1","1","Etiquetas multilingues relativas aos gases de estufa fluorados"]
["Refrigerant","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Carga","","","kg","1.0","1.0","1.20","1.3"]
["","Tipo","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","780","780","780","790"]
["","","Aquecimento","Super baixa","rpm","740","740","740","780"]
["Limites de funcionamento","Arrefecimento","Ambiente","Máx.","° CBs","46","46","46","46"]
["","","","Mín.","° CBs","-10","-10","-10","-10"]
["","Aquecimento","Ambiente","Máx.","° CBh","18","18","18","18"]
["","","","Mín.","° CBh","-15","-15","-15","-15"]
["Ligações de tubagem","Diferença de nível","IU - OU","Máx.","m","","","15"]
["","Carga de refrigerante adicional","","","kg/m","","","0,020 (para comprimento de tubagem superior a 10m)"]
["Dimensões","Unidade","","Largura","mm","765","765","765","765"]
["","","","Profundidade","mm","285","285","285","285"]
["","","","Altura","mm","550","550","550","550"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Peso","Unidade","","","kg","34","34","34","39"]
["Ventoinha","Caudal de ar","Aquecimento","Super baixa","cfm","904","904","904","960"]
["","","","Super baixa","m³/min","25.6","25.6","25.6","27.2"]
["","","Arrefecimento","Super baixa","m³/min","30.1","30.1","30.1","30.6"]
["","","","Super baixa","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequência","","","Hz","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Contém gases fluorados com efeito de estufa","(4) - Contém gases fluorados com efeito de estufa","(4) - Contém gases fluorados com efeito de estufa","(4) - Contém gases fluorados com efeito de estufa"]
["Ventilador","Caudal de ar","Arrefecimento","Super baixa","m³/min","","","","","48.9","45.0"]
["","","Aquecimento","Super baixa","m³/min","","","","","43.1","46.3"]
["","","","Super baixa","cfm","","","","","1727","1589"]
["","","Aquecimento","Super baixa","cfm","","","","","1522","1635"]
["Dimensões","Unidade","","Altura","mm","","","","","735","735"]
["","","","Largura","mm","","","","","825","825"]
["","","","Profundidade","mm","","","","","300","300"]
["Peso","Unidade","","","kg","","","","","47","48"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","","","","","670"]
["","","Aquecimento","Super baixa","rpm","","","","","670"]
["Compressor","Tipo","","","","","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","","","","","-10","-10"]
["","","","Máx.","° CBs","","","","","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","","","","","-15","-15"]
["","","","Máx.","° CBh","","","","","18","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","","","","48","49"]
["","","","B","dBA","","","","","44","46"]
["","Aquecimento","","Alto","dBA","","","","","48","49"]
["","","","B","dBA","","","","","45","46"]
["Fluido frigorigéneo","Tipo","","","","","","","","R-410A","R-410A"]
["","Carga","","","kg","","","","","1.7","1.5"]
["","Carga","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","","","","","30","30"]
["","Carga de refrigerante adicional","","","kg/m","","","","","0,020 (para comprimento de tubagem superior a 10m)","0,020 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","","","","","20.0","20"]
["Acessórios standard","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Alimentação elétrica","Fase","","","","","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","","","","50","50"]
["","Tensão","","","V","","","","","220-230-240","220-230-240"]
["Notas","","","","","","","","","","(1) - 230V"]