{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","","","48"]
["","Arrefecimento","","Alto","dBA","","","48"]
["Acessórios standard","Manual de instalação","","","","","","1"]
["","Etiqueta da carga de refrigerante","","","","","","1"]
["","Etiquetas multilingues relativas aos gases de estufa fluorados","","","","","","1"]
["","Tampão de drenagem (apenas modelos com bombas de calor)","","","","","","1"]
["Fluido frigorigéneo","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Carga","","","kg","","","1.2"]
["","Type","","","","","","R-410A"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","","","780"]
["","","Aquecimento","Super baixa","rpm","","","740"]
["Limite de funcionamento","Arrefecimento","Ambiente","Máx.","° CBs","","","46"]
["","","","Mín.","° CBs","","","-10"]
["","Aquecimento","Ambiente","Máx.","° CBh","","","18"]
["","","","Mín.","° CBh","","","-15"]
["Piping connections","Diferença de nível","IU - OU","Máx.","m","","","15"]
["","Carga de refrigerante adicional","","","kg/m","","","0,02 (para comprimento de tubagem superior a 10m)"]
["Dimensões","Unidade","","Width","mm","","","765"]
["","","","Depth","mm","","","285"]
["","","","Altura","mm","","","550"]
["Compressor","Tipo","","","","","","Compressor oscilante hermético"]
["Peso","Unidade","","","kg","","","34"]
["Ventilador","Caudal de ar","Aquecimento","Super baixa","cfm","","","904"]
["","","","Super baixa","m³/min","","","25.6"]
["","","Arrefecimento","Super baixa","m³/min","","","30.1"]
["","","","Super baixa","cfm","","","1,063"]
["Power supply","Fase","","","","","","1~"]
["","Frequência","","","Hz","","","50"]
["","Tensão","","","V","","","220-240"]
["Notas","","","","","","","(1) - SL: O nível de ventilador silencioso da definição da taxa do caudal de ar"]
["Ventilador","Caudal de ar","Arrefecimento","Super baixa","m³/min","30.1","30.1"]
["","","Aquecimento","Super baixa","m³/min","25.6","25.6"]
["","","","Super baixa","cfm","1063","1063"]
["","","Aquecimento","Super baixa","cfm","904","904"]
["Dimensões","Unidade","","Altura","mm","550","550"]
["","","","Largura","mm","765","765"]
["","","","Profundidade","mm","285","285"]
["Peso","Unidade","","","kg","34","34"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","780","780"]
["","","Aquecimento","Super baixa","rpm","740","740"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10","-10"]
["","","","Máx.","° CBs","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15","-15"]
["","","","Máx.","° CBh","18","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","46","46"]
["","Aquecimento","","Alto","dBA","47","47"]
["Fluido frigorigéneo","Tipo","","","","R-410A","R-410A"]
["","Carga","","","kg","1.0","1.0"]
["","Carga","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20","20"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","15","15"]
["Acessórios standard","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]
["Notas","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Acessórios standard","Drain plug (only heat pump models)","","","","","1"]