{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-A"]
[]
[]
[]
[]
["","","","","","RXTM30A2V1B","RXTM40A2V1B"]
["Dimensões","Unidade","","Altura","mm","605","605"]
["","","","Largura","mm","930","930"]
["","","","Profundidade","mm","376","376"]
["Peso","Unidade","","","kg","42","42"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","800","800"]
["","","Aquecimento","Super baixa","rpm","400","400"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10","-10"]
["","","","Máx.","° CBs","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-31","-31"]
["","","","Máx.","° CBh","18","18"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","48","48"]
["","Aquecimento","","Nom.","dBA","49.0","49.0"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","0.97","0.97"]
["","Carga","","","tCO2Eq","0.66","0.66"]
["","GWP","","","","675.0","675.0"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20","20"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","15.0","15.0"]
["Acessórios standard","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]