{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B9","RXZ35NV1B","RXZ50NV1B9","RXZ50NV1B"]
["Dimensões","Unidade","","Altura","mm","693","693","693","693","693","693"]
["","","","Largura","mm","795","795","795","795","795","795"]
["","","","Profundidade","mm","300","300","300","300","300","300"]
["Peso","Unidade","","","kg","50","50","50","50","50","50"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","-10","-10","-10","-10","-10","-10"]
["","","","Máx.","°CBs","43","43","43","43","43","43"]
["","Aquecimento","Ambiente","Mín.","° CBh","-20","-20","-20","-20","-20","-20"]
["","","","Máx.","° CBh","18","18","18","18","18","18"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","46","46","48","48","49","49"]
["","Aquecimento","","Alto","dBA","46","46","48","48","50","50"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","1.34","1.34","1.34","1.34","1.34","1.34"]
["","Carga","","","tCO2Eq","0.9","0.9","0.9","0.9","0.9","0.9"]
["","GWP","","","","675","675","675","675","675","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","10","10","10","10","10","10"]
["","Diferença de nível","IU - OU","Máx.","m","8","8","8","8","8","8"]
["Acessórios standard","Installation manual","","","","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]