{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensões","Unidade","","Altura","mm","870","870"]
["","","","Largura","mm","1,100","1,100"]
["","","","Profundidade","mm","460","460"]
["Peso","Unidade","","","kg","117","117"]
["Compressor","Tipo","","","","Compressor scroll hermeticamente vedado","Compressor scroll hermeticamente vedado"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-20","-20"]
["","","","Máx.","° CBs","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-20","-20"]
["","","","Máx.","° CBh","15","15"]
["Nível de potência sonora","Arrefecimento","","","dBA","73","76"]
["","Aquecimento","","","dBA","76 (1)","79 (1)"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","53","57"]
["","Aquecimento","","Nom.","dBA","60","63"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","GWP","","","","675","675"]
["Ligações de tubagem","Líquido","","DE","mm","9.52","9.52"]
["","Gás","","DE","mm","22.2","22.2"]
["","Comprimento da tubagem","Máx.","OU - IU","m","100","100"]
["","","Sistema","Sem carga","m","30","30"]
["","Carga de refrigerante adicional","","","kg/m","Consultar manual de instalação","Consultar manual de instalação"]
["Acessórios standard","Manual de instalação","","","","1","1"]
["","Precauções gerais de segurança","","","","1","1"]
["","Atilhos","","","","2","2"]
["","Etiqueta autocolante de gás F","","","","1","1"]
["","Tubos de ligação","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frequência","","","Hz","50","50"]
["","Tensão","","","V","380-415","380-415"]
["Corrente - 50Hz","Amperagem máxima de fusíveis (MFA)","","","A","20","20"]
["Notas","","","","","(1) - De acordo com ENER Lote 21","(1) - De acordo com ENER Lote 21"]