{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Dimensões","Unidade","","Altura","mm","734","734","734"]
["","","","Largura","mm","870","870","870"]
["","","","Profundidade","mm","373","373","373"]
["Peso","Unidade","","","kg","52","52","52"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-20","-20","-20"]
["","","","Máx.","° CBs","52","52","52"]
["","Aquecimento","Ambiente","Mín.","° CBh","-21","-21","-21"]
["","","","Máx.","° CBh","18","18","18"]
["Nível de potência sonora","Arrefecimento","","","dBA","62","63","64"]
["","Aquecimento","","","dBA","62","63","64"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","48","49","50"]
["","Aquecimento","","Nom.","dBA","48","49","50"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32"]
["","Carga","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Carga","","","tCO2Eq","1.05","1.05","1.05"]
["Ligações de tubagem","Líquido","","DE","mm","6.35","6.35","6.35"]
["","Gás","","DE","mm","9.52","12.7","12.7"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","50","50","50"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 30m)","0,02 (para comprimento de tubagem superior a 30m)","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","30","30","30"]
["Acessórios standard","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240"]
["Notas","","","","","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","(2) - Consulte o esquema separado para conhecer os dados eléctricos","(2) - Consulte o esquema separado para conhecer os dados eléctricos","(2) - Consulte o esquema separado para conhecer os dados eléctricos"]
["","","","","","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa"]
["Acessórios standard","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]