{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Nível de pressão sonora","Aquecimento","","Nom.","dBA","","","","52"]
["","Arrefecimento","","Nom.","dBA","","","","51"]
["Acessórios standard","Atilhos","","","","","","","2"]
["","Manual de instalação","","","","","","","1"]
["","Etiqueta de refrigerante para norma de gás F","","","","","","","1"]
["","Precauções gerais de segurança","","","","","","","1"]
["","Etiqueta energética LOT10","","","","","","","1"]
["Fluido frigorigéneo","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Carga","","","kg","","","","3.75"]
["","Type","","","","","","","R-32"]
["Piping connections","Liquid","","OD","mm","","","","9.52"]
["","Comprimento da tubagem","Máx.","OU - IU","m","","","","85"]
["","","Sistema","Sem carga","m","","","","40"]
["","","","Equivalente","m","","","","100"]
["","Gás","","OD","mm","","","","15.9"]
["","Diferença de nível","IU - IU","Máx.","m","","","","0.5"]
["","","IU - OU","Máx.","m","","","","30.0"]
["","Carga de refrigerante adicional","","","kg/m","","","","Consultar manual de instalação"]
["Nível de potência sonora","Arrefecimento","","","dBA","","","","70"]
["","Aquecimento","","","dBA","","","","70 (1)"]
["Compressor","Tipo","","","","","","","Compressor oscilante hermético"]
["Dimensões","Unidade","","Width","mm","","","","940"]
["","","","Depth","mm","","","","320"]
["","","","Altura","mm","","","","1,430"]
["Peso","Unidade","","","kg","","","","92"]
["Power supply","Fase","","","","","","","1~"]
["","Frequência","","","Hz","","","","50"]
["","Tensão","","","V","","","","220-240"]
["Notas","","","","","","","","(1) - De acordo com ENER Lote 21"]
["","","","","","","","","(2) - Norma técnica europeia/internacional que define os limites para correntes harmónicas produzidas por equipamento ligado a um sistema público de baixa tensão com corrente de entrada superior a 16A e ≤ 75A por fase."]
["","","","","","","","","(3) - Ssc: potência de curto-circuito"]
["","","","","","","","","(4) - Norma técnica europeia/internacional que define os limites para correntes harmónicas produzidas por equipamento ligado a um sistema público de baixa tensão com corrente de entrada ≤ 16 A por fase."]
["Dimensões","Unidade","","Altura","mm","990","1430","1430"]
["","","","Largura","mm","940","940","940"]
["","","","Profundidade","mm","320","320","320"]
["Peso","Unidade","","","kg","70","92","92"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-20","-20","-20"]
["","","","Máx.","° CBs","52","52","52"]
["","Aquecimento","Ambiente","Mín.","° CBh","-20","-20","-20"]
["","","","Máx.","° CBh","18.0","18.0","18.0"]
["Nível de potência sonora","Arrefecimento","","","dBA","64","66","69"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","46","47","50"]
["","Aquecimento","","Nom.","dBA","49","51","52"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32"]
["","Carga","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Carga","","","tCO2Eq","1.99","2.53","2.53"]
["Ligações de tubagem","Líquido","","DE","mm","9.52","9.52","9.52"]
["","Gás","","DE","mm","15.9","15.9","15.9"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","55","85","85"]
["","","Sistema","Equivalente","m","75","100","100"]
["","","","Sem carga","m","40","40","40"]
["","Carga de refrigerante adicional","","","kg/m","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação"]
["","Diferença de nível","IU - OU","Máx.","m","30.0","30.0","30.0"]
["","","IU - IU","Máx.","m","0.5","0.5","0.5"]
["Acessórios standard","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Alimentação elétrica","Fase","","","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240"]
["Corrente - 50 Hz","Amperagem máxima de fusíveis (MFA)","","","A","20","32","32"]
["Nível de potência sonora","Aquecimento","","","dBA","","","69 (1)"]
["Notas","","","","","","","(1) - De acordo com ENER Lote 21"]