{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":13,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NY1"]
[]
[]
[]
[]
["","","","","","RZAG71N2Y1B","RZAG71N7Y1B","RZAG100N7Y1B","RZAG100N2Y1B","RZAG125N7Y1B","RZAG125N2Y1B","RZAG140N7Y1B","RZAG140N2Y1B"]
["Dimensões","Unidade","","Altura","mm","870","870","870","870","870","870","870","870"]
["","","","Largura","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Profundidade","mm","460","460","460","460","460","460","460","460"]
["Peso","Unidade","","","kg","81","81","85","85","94","94","94","94"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Máx.","° CBs","52","52","52","52","52","52","52","52"]
["","Aquecimento","Ambiente","Mín.","° CBh","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Máx.","° CBh","18","18","18","18","18","18","18","18"]
["Nível de potência sonora","Arrefecimento","","","dBA","64","64","66","66","69","69","70","70"]
["","Aquecimento","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Aquecimento","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","3.20","3.2","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["","Carga","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Ligações de tubagem","Líquido","","DE","mm","10","10","10","10","10","10","10","10"]
["","Gás","","DE","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","55","55","85","85","85","85","85","85"]
["","","Sistema","Equivalente","m","75","75","100","100","100","100","100","100"]
["","","","Sem carga","m","40","40","40","40","40","40","40","40"]
["","Carga de refrigerante adicional","","","kg/m","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação","Consultar manual de instalação"]
["","Diferença de nível","IU - OU","Máx.","m","30","30","30","30","30","30","30","30"]
["","","IU - IU","Máx.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Acessórios standard","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Alimentação elétrica","Fase","","","","3~","3~","3~","3~","3~","3~","3~","3~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50","50","50","50","50"]
["","Tensão","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Corrente - 50 Hz","Amperagem máxima de fusíveis (MFA)","","","A","16","16","16","16","16","16","16","16"]
["Notas","","","","","","","","","(1) - De acordo com ENER Lote 21","(1) - De acordo com ENER Lote 21","(1) - De acordo com ENER Lote 21","(1) - De acordo com ENER Lote 21"]