{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensões","Unidade","","Altura","mm","1,680"]
["","","","Largura","mm","930"]
["","","","Profundidade","mm","765"]
["Peso","Unidade","","","kg","183.0"]
["Compressor","Type","","","","Compressor scroll hermeticamente vedado"]
["Limites de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","-5.0"]
["","","","Máx.","°CBs","46.0"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15.0"]
["","","","Máx.","° CBh","15.0"]
["Nível de potência sonora","Arrefecimento","","","dBA","78.0"]
["","Aquecimento","","","dBA","78.0"]
["Fluido frigorigéneo","Tipo","","","","R-410A"]
["","Carga","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Ligações de tubagem","Líquido","","DE","mm","9.52"]
["","Gás","","DE","mm","22.2"]
["","Comprimento da tubagem","Máx.","OU - IU","m","100"]
["","","Sistema","Sem carga","m","30"]
["Acessórios standard","Manual de instalação","","","","1"]
["","Tubos de ligação","","","","4"]
["Power supply","Fase","","","","3N~"]
["","Frequência","","","Hz","50"]
["","Tensão","","","V","380-415"]
["Corrente - 50Hz","Amperagem máxima de fusíveis (MFA)","","","A","25"]
["Notas","","","","","(1) - A fonte de alimentação para a unidade interior FDQ é separada"]
["","","","","","(2) - Consulte os esquemas separados para conhecer os dados eléctricos"]
["Dimensões","Unidade","","Altura","mm","","1680"]
["","","","Largura","mm","","930"]
["","","","Profundidade","mm","","765"]
["Peso","Unidade","","","kg","","184.0"]
["Compressor","Tipo","","","","","Compressor scroll hermeticamente vedado"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","","-5.0"]
["","","","Máx.","°CBs","","46.0"]
["","Aquecimento","Ambiente","Mín.","° CBh","","-15.0"]
["","","","Máx.","° CBh","","15.0"]
["Nível de potência sonora","Arrefecimento","","","dBA","","78.0"]
["","Aquecimento","","","dBA","","78.0"]
["Fluido frigorigéneo","Carga","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Carga","","","tCO2Eq","","19.4"]
["Ligações de tubagem","Líquido","","DE","mm","","12.70"]
["","Gás","","DE","mm","","22.2"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","","100"]
["","","Sistema","Sem carga","m","","30"]
["Acessórios standard","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Alimentação eléctrica","Frequência","","","Hz","","50"]
["Corrente - 50 Hz","Amperagem máxima de fusíveis (MFA)","","","A","","25"]