{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLTRH"]
[]
[]
[]
[]
["","","","","WLTRH."]
["Número máximo de unidades interiores conectáveis","","","","0"]
["Número máximo de unidades exteriores conectáveis @","","","","0"]
["Envolvente","Cor","","","Branco"]
["Estrutura","Tampa do botão","","","Não"]
["","LED de funcionamento","Cor","","Verde"]
["Dimensões","Unidade","Altura","mm","75"]
["","","Largura","mm","60.0"]
["","","Profundidade","mm","25.0"]
["","Unidade embalada","Altura","mm","380"]
["","","Largura","mm","305"]
["","","Profundidade","mm","195"]
["Peso","Unidade","","kg","0.036"]
["Acondicionamento","Material","","","Cartão"]
["","Peso","","kg","0.0084"]
["Temperatura ambiente","Funcionamento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["","Armazenamento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["","Temperatura ambiente-=-Humidade relativa <-=-%","","%","100"]
["Instalação","","","","Instalação no interior"]